,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AUUW24GAE","UU24W U44",U4,"1,500 x 1",Twin Rotary,"9,700 ~ 23,200 ~ 26,600",2.84 ~ 6.80 ~ 7.80,37-13/32 x 32-27/32 x 13,950 x 834 x 330,Electronic Expansion Valve,2048.33 x 1,58 x 1,124 x 1,BLDC,Axial,"10,900 ~ 27,300 ~ 30,000",3.20 ~ 8.00 ~ 8.80,AUUW24GAE,56.1 ,123.6,5/8,15.88,3/8,9.52,2,2.22,"1, 220-240, 50",3C x 2.5 (12),"2,000 ",15.88,9.52,R410A,8.9,9.7,67,-,48,52,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 64.4,SingleCAC_StandardInverter
"AUUW30GAE","UU30W U44",U4,"2,137 x 1",Twin Rotary,"10,900 ~ 27,300 ~ 30,000",3.20 ~ 8.00 ~ 8.80,37-13/32 x 32-27/32 x 13,950 x 834 x 330,Electronic Expansion Valve,2048.33 x 1,58 x 1,124 x 1,BLDC,Axial,"12,300 ~ 30,700 ~ 33,800",3.60 ~ 9.00 ~ 9.90,AUUW30GAE,58.0 ,127.8,5/8,15.88,3/8,9.52,2.49,2.72,"1, 220-240, 50",3C x 2.5 (12),"2,000 ",15.88,9.52,R410A,10.8,11.8,68,-,48,52,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 64.4,SingleCAC_StandardInverter
"AUUW246D2","",U4,"2,137 x 1",Twin Rotary,"9,500 ~ 24,200 ~ 26,600",2.8 ~ 7.1 ~ 7.8,37-13/32 x 32-27/32 x 13,950 x 834 x 330,Electronic Expansion Valve,2048.33 x 1,58 x 1,124 x 1,BLDC,Propeller,"10,900 ~ 27,300 ~ 30,000",3.2 ~ 8.0 ~ 8.8,AUUW246D2,60.0 ,132.3,5/8,15.88,3/8,9.52,1.99,2.26,"1, 220-240, 50",3C x 2.5 (12),"2,000 ",15.88,9.52,R410A,8.7,9.8,62,-,48,52,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 64.4,SingleCAC_StandardInverter

