,Model name (Buyer)##other##,URL##OTHER##,Type##OTHER##,Sound Pressure Level Heating(dB)##OTHER##,Sound Pressure Level Cooling(dB)##OTHER##,Sound Power Level (dB(A))##OTHER##,Running Current (A)##OTHER##,Refrigerant Type##OTHER##,Refrigerant Suction Gas Connection Radius##PIPE_SIZE##MILLIMETERS,Refrigerant Suction Gas Connection Offset Top##LENGTH##MILLIMETERS,Refrigerant Suction Gas Connection Offset back##LENGTH##MILLIMETERS,Refrigerant Gas Connection Diameter##PIPE_SIZE##MILLIMETERS,Refrigerant Liquid Connection Radius##PIPE_SIZE##MILLIMETERS,Refrigerant Liquid Connection Offset Top##LENGTH##MILLIMETERS,Refrigerant Liquid Connection Offset back##LENGTH##MILLIMETERS,Refrigerant Liquid Connection Diameter##PIPE_SIZE##MILLIMETERS,Power and Communication Cable##OTHER##,Power Supply (Ph_V_Hz)##OTHER##,Power Input (Heating)(W)##OTHER##,Power Input (Cooling)(W)##OTHER##,Pipe Connection_Liquid Side (mm)##OTHER##,Pipe Connection_Liquid Side (inch)##OTHER##,Pipe Connection_Gas Side (mm)##OTHER##,Pipe Connection_Gas Side (inch)##OTHER##,Pipe Connection_Drain Side (mm)##OTHER##,Pipe Connection_Drain Side (inch)##OTHER##,Net Weight (lbs)##OTHER##,Net Weight (kg)##OTHER##,Model name (Factory)##OTHER##,Model##OTHER##,Heating Capacity (kW)##OTHER##,Heating Capacity (Btu/h)##OTHER##,Fan Type##OTHER##,Fan Motor Type##OTHER##,Fan Motor Output (W)##OTHER##,Dimensions (WxHxD)(mm)##OTHER##,Dimensions (WxHxD)(inch)##OTHER##,Cooling Capacity (kW)##OTHER##,Cooling Capacity (Btu/h)##OTHER##,Condensate Drain Connection Radius##PIPE_SIZE##MILLIMETERS,Condensate Drain Connection Offset Top##LENGTH##MILLIMETERS,Condensate Drain Connection Offset back##LENGTH##MILLIMETERS,Condensate Drain Connection Diameter##PIPE_SIZE##MILLIMETERS,Chassis name##OTHER##,Air Flow Rate (H/M/L)(CMM)##OTHER##,Air Flow Rate (H/M/L)(CFM)##OTHER##
ZMNW09GAF10,MA09R NF1,http://partner.lge.com/global,ArtCool,38 / 32 / 27,38 / 32 / 27,52,0.2,R32,4.760000000000,30.000000000000,14.000000000000,9.520000000000,3.175000000000,44.000000000000,14.000000000000,6.350000000000,4C x 0.75 (18),"1,220-240, 50 / 1, 220, 60",-,40 x 1,6.35,1/4,9.52,3/8,21.5,-,33.1,15,ZMNW09GAF10,,2.5,"9,000",Turbo Fan,BLDC,24 x 1,600 x 600 x 145,23-5/8 x 23-5/8 x 5-23/32,2.5,"9,000",10.750000000000,33.000000000000,30.000000000000,21.500000000000,SF,7.7 / 5.9 / 4.4,272 / 208 / 155
ZMNW12GAF10,MA12R NF1,http://partner.lge.com/global,ArtCool,44 / 38 / 32,44 / 38 / 32,54,0.2,R32,4.760000000000,30.000000000000,14.000000000000,9.520000000000,3.175000000000,44.000000000000,14.000000000000,6.350000000000,4C x 0.75 (18),"1,220-240, 50 / 1, 220, 60",-,40 x 1,6.35,1/4,9.52,3/8,21.5,-,33.1,15,ZMNW12GAF10,,3.5,"12,000",Turbo Fan,BLDC,24 x 1,600 x 600 x 145,23-5/8 x 23-5/8 x 5-23/32,3.5,"12,000",10.750000000000,33.000000000000,30.000000000000,21.500000000000,SF,8.9 / 7.3 / 5.6,314 / 258 / 198
