,Model name (Buyer)##other##,Width offset mid##LENGTH##MILLIMETERS,Width##LENGTH##MILLIMETERS,URL##OTHER##,Type##OTHER##,Sound Pressure Level Heating(dB)##OTHER##,Sound Pressure Level Cooling(dB)##OTHER##,Sound Power Level (dB(A))##OTHER##,Running Current (A)##OTHER##,Refrigerant Type##OTHER##,Refrigerant Gas Connection Radius##PIPE_SIZE##MILLIMETERS,Refrigerant Gas Connection Offset Top##LENGTH##MILLIMETERS,Refrigerant Gas Connection Offset Front##LENGTH##MILLIMETERS,Refrigerant Gas Connection Diameter##PIPE_SIZE##MILLIMETERS,Refrigerant Liquid Connection Radius##PIPE_SIZE##MILLIMETERS,Refrigerant Liquid Connection Offset Top##LENGTH##MILLIMETERS,Refrigerant Liquid Connection Offset Front##LENGTH##MILLIMETERS,Refrigerant Liquid Connection Diameter##PIPE_SIZE##MILLIMETERS,Power and Communication Cable##OTHER##,Power Supply (Ph_V_Hz)##OTHER##,Power Input (Heating)(W)##OTHER##,Power Input (Cooling)(W)##OTHER##,Pipe Connection_Liquid Side (mm)##OTHER##,Pipe Connection_Liquid Side (inch)##OTHER##,Pipe Connection_Gas Side (mm)##OTHER##,Pipe Connection_Gas Side (inch)##OTHER##,Pipe Connection_Drain Side (mm)##OTHER##,Pipe Connection_Drain Side (inch)##OTHER##,Net Weight (lbs)##OTHER##,Net Weight (kg)##OTHER##,Model name (Factory)##OTHER##,Model##OTHER##,Length offset top mid##LENGTH##MILLIMETERS,Length offset top left##LENGTH##MILLIMETERS,Length offset mid##LENGTH##MILLIMETERS,Length##LENGTH##MILLIMETERS,Height offset mid##LENGTH##MILLIMETERS,Height offset top##LENGTH##MILLIMETERS,Height offset bottom##LENGTH##MILLIMETERS,Height##LENGTH##MILLIMETERS,Heating Capacity (kW)##OTHER##,Heating Capacity (Btu/h)##OTHER##,Hanger offset Height##LENGTH##MILLIMETERS,Fan Type##OTHER##,Fan Motor Type##OTHER##,Fan Motor Output (W)##OTHER##,Dimensions (WxHxD)(mm)##OTHER##,Dimensions (WxHxD)(inch)##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Cooling Capacity (kW)##OTHER##,Cooling Capacity (Btu/h)##OTHER##,Condensate Drain Connection Radius##PIPE_SIZE##MILLIMETERS,Condensate Drain Connection Diameter##PIPE_SIZE##MILLIMETERS,Chassis name##OTHER##,Bottom offset width##LENGTH##MILLIMETERS,Bottom offset Length##LENGTH##MILLIMETERS,Air Suction grill Width##LENGTH##MILLIMETERS,Air Suction grill Length##LENGTH##MILLIMETERS,Air Flow Rate (H/M/L)(CMM)##OTHER##,Air Flow Rate (H/M/L)(CFM)##OTHER##,Air Discharge grill Width##LENGTH##MILLIMETERS,Air Discharge grill Length##LENGTH##MILLIMETERS
ZMNW09GTUA0,MT09R NU1,450.000000000000,500.000000000000,http://partner.lge.com/global,CST 1Way,36 / 34 / 32,36 / 34 / 32,54,0.2,R32,4.760000000000,97.000000000000,229.000000000000,9.520000000000,3.175000000000,90.000000000000,293.000000000000,6.350000000000,4C x 0.75 (18),"1,220-240, 50 / 1, 220, 60",-,20 x 1,6.35,1/4,9.52,3/8,32,-,25.8,11.7,ZMNW09GTUA0,,860.000000000000,35.600000000000,961.200000000000,1100.000000000000,34.000000000000,170.000000000000,34.000000000000,200.000000000000,2.5,"9,000",132.000000000000,Cross Flow Fan,BLDC,20 x 1,860 x 132 x 450,33-27/32 x 5-3/16 x17-23/32,0.000000000000,2.5,"9,000",12.700000000000,32.000000000000,TU,42.000000000000,57.000000000000,75.000000000000,955.000000000000,7.5 / 7.3 / 6.8,265 / 258 / 240,224.000000000000,955.000000000000
ZMNW12GTUA0,MT11R NU1,450.000000000000,500.000000000000,http://partner.lge.com/global,CST 1Way,37 / 36 / 33,37 / 36 / 33,57,0.2,R32,4.760000000000,97.000000000000,229.000000000000,9.520000000000,3.175000000000,90.000000000000,293.000000000000,6.350000000000,4C x 0.75 (18),"1,220-240, 50 / 1, 220, 60",-,20 x 1,6.35,1/4,9.52,3/8,32,-,25.8,11.7,ZMNW12GTUA0,,860.000000000000,35.600000000000,961.200000000000,1100.000000000000,34.000000000000,170.000000000000,34.000000000000,200.000000000000,3.5,"12,000",132.000000000000,Cross Flow Fan,BLDC,20 x 1,860 x 132 x 450,33-27/32 x 5-3/16 x17-23/32,0.000000000000,3.5,"12,000",12.700000000000,32.000000000000,TU,42.000000000000,57.000000000000,75.000000000000,955.000000000000,8.1 / 7.4 / 7.0,286 / 261 / 247,224.000000000000,955.000000000000
