,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZTNW24GPLA0,CT24R NP0,-,17.0 / 15.0 / 13.0,TP,32,23202.56,6.80,-,840 × 204 × 840,50.25 x 1,BLDC,Turbo Fan,27297.13,8.00,ZTNW24GPLA0,20.5,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,-,-,"1, 220-240, 50",15.88 ,9.52 ,R32,0.6,53,38 / 36 / 34,-,4way CST
ZTNW30GPLA0,UT30R NP0,-,19.0 / 17.0 / 15.0,TP,32,30000,8.8,-,840 × 204 × 840,50.25 x 1,BLDC,3D Turbo Fan,30000,8.8,ZTNW30GPLA0,20.5,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,-,-,"1, 220-240, 50",15.88 ,9.52 ,R32,-,58,40.0 / 37.0 / 35.0,-,4way CST


