,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ZBNW18GM1A0","CM18R N10",-,16.5 / 14.5 / 13.0,M1,32,-,1.80 ~ 5.00 ~ 5.30,-,900 × 270 × 700,136.5 x 1,BLDC,Sirocco Fan,-,1.70 ~ 5.20 ~ 6.00,ZBNW18GM1A0,26.5,-,-,32,1/2,12.7 ,1/4,6.35 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",12.7 ,6.35 ,R32,0.57,59,34 / 32 / 30,-,Duct Mid Static
"ZBNW24GM1A0","CM24R N10",-,18.0 / 16.5 / 14.5,M1,32,-,2.7 / 6.8 / 7.4,-,900 × 270 × 700,136.5 x 1,BLDC,Sirocco Fan,-,1.9 / 7.5 / 8.2,ZBNW24GM1A0,26.5,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,0.66,60,35 / 34 / 32,-,Duct Mid Static
"ZBNW30GM1A0","UM30R N10",-,22.0 / 20.0 / 18 .0,M1,32,-,3.0 / 7.5 / 8.2,-,900 × 270 × 700,136.5 x 1,BLDC,Sirocco Fan,-,2.0 / 8.0 / 8.4,ZBNW30GM1A0,26.5,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,0.66,62,37 / 35 / 34,-,Duct Mid Static

