,Model name (Buyer)##other##,URL##OTHER##,Type##OTHER##,Sound Pressure Level Heating(dB)##OTHER##,Sound Pressure Level Cooling(dB)##OTHER##,Sound Power Level (dB(A))##OTHER##,Running Current (A)##OTHER##,Refrigerant Type##OTHER##,Refrigerant Gas Connection Radius##LENGTH##MILLIMETERS,Refrigerant Liquid Connection Radius##LENGTH##MILLIMETERS,Refrigerant Liquid Connection Diameter##PIPE_SIZE##MILLIMETERS,Refrigerant Gas Connection Diameter##PIPE_SIZE##MILLIMETERS,Power and Communication Cable##OTHER##,Power Supply (Ph_V_Hz)##OTHER##,Power Input (Heating)(W)##OTHER##,Power Input (Cooling)(W)##OTHER##,Pipe Connection_Liquid Side (mm)##OTHER##,Pipe Connection_Liquid Side (inch)##OTHER##,Pipe Connection_Gas Side (mm)##OTHER##,Pipe Connection_Gas Side (inch)##OTHER##,Pipe Connection_Drain Side (mm)##OTHER##,Pipe Connection_Drain Side (inch)##OTHER##,Net Weight (lbs)##OTHER##,Net Weight (kg)##OTHER##,Model name (Factory)##OTHER##,Heating Capacity (kW)##OTHER##,Heating Capacity (Btu/h)##OTHER##,Fan Type##OTHER##,Fan Motor Type##OTHER##,Fan Motor Output (W)##OTHER##,Dimensions (WxHxD)(mm)##OTHER##,Dimensions (WxHxD)(inch)##OTHER##,Cooling Capacity (kW)##OTHER##,Cooling Capacity (Btu/h)##OTHER##,Condensate Drain Connection Radius##LENGTH##MILLIMETERS,Condensate Drain Connection Diameter##PIPE_SIZE##MILLIMETERS,Chassis name##OTHER##,Air Flow Rate (H/M/L)(CMM)##OTHER##,Air Flow Rate (H/M/L)(CFM)##OTHER##
"ZVNW18GM1A0","UV18R N10",http://partner.lge.com/global,Ceiling Suspended,-,42 / 40 / 39,55,1,R32,6.350000000000,3.175000000000,6.350000000000,12.700000000000,4C x 0.75,"1, 220-240, 50 / 1, 220, 60",-,-,6.35,1/4,12.7,1/2,21.5,-,-,27.3,ZVNW18GM1A0,2.00 ~ 5.20 ~ 6.30,"6,824 ~ 17,743 ~ 21,496",Cross flow Fan,BLDC,105.4 x 1,"1,200 x 235 x 690",-,1.92 ~ 5.00 ~ 6.00,"6,551 ~ 17,060 ~ 20,472",10.750000000000,21.500000000000,VM1,13.0 / 12.0 / 11.0,-
"ZVNW24GM1A0","UV24R N10",http://partner.lge.com/global,Ceiling Suspended,-,46 / 45 / 43,61,1,R32,7.940000000000,4.760000000000,9.520000000000,15.880000000000,4C x 0.75,"1, 220-240, 50 / 1, 220, 60",-,-,9.52,3/8,15.88,5/8,21.5,-,-,28,ZVNW24GM1A0,3.00 ~ 7.50 ~ 8.30,"10,236 ~ 25,591 ~ 28,320",Cross flow Fan,BLDC,105.4 x 1,"1,200 x 235 x 690",-,2.80 ~ 6.80 ~ 7.48,"9,553 ~ 23,202 ~ 25,522",10.750000000000,21.500000000000,VM1,16.0 / 15.0 / 14.0,-
