,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"AMNH09GTUC0",MT09AH NU1,265 / 258 / 240,7.5 / 7.3 / 6.8,TU,32,"5,400 ~ 9,000 ~ 10,800",1.6 ~ 2.6 ~ 3.2,33-27/32 x 5-3/16 x 17-23/32,860 x 132 x 450,20 x 1,BLDC,Cross Flow Fan,"6,480 ~ 10,800 ~ 12,420",1.9 ~ 3.2 ~ 3.6,AMNH09GTUC0,13.5,29.8,1-1/4,32.0,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),20 x 1,-,"220-240, 1, 50 / 220, 1, 60",9.52,6.35,R410A,0.2,54,36 / 34 / 32,-,1Way CST
"AMNH12GTUC0",MT11AH NU1,286 / 261 / 247,8.1 / 7.4 / 7.0,TU,32,"7,200 ~ 12,000 ~ 14,400",2.1 ~ 3.5 ~ 4.2,33-27/32 x 5-3/16 x 17-23/32,860 x 132 x 450,20 x 1,BLDC,Cross Flow Fan,"8,640 ~ 14,400 ~ 16,560",2.5 ~ 4.2 ~ 4.9,AMNH12GTUC0,13.5,29.8,1-1/4,32.0,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),20 x 1,-,"220-240, 1, 50 / 220, 1, 60",9.52,6.35,R410A,0.2,57,37 / 36 / 33,-,1Way CST

