,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ZBNW48GM3A0","UM48R N30",-,40 / 34 / 28,M3,32,-,5.5 ~ 13.4 ~ 16.0,-,"1,250 × 360 × 700",290 x 1,BLDC,Sirocco Fan,-,6.1 ~ 15.5 ~ 18.0,ZBNW48GM3A0,43.5,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,2.5,65,40 / 38 / 36,-,Duct Mid Static
"ZBNW60GM3A0","UM60R N30",-,50 / 45 / 40,M3,32,-,5.9 ~ 15.0 ~ 16.3,-,"1,250 × 360 × 700",290 x 1,BLDC,Sirocco Fan,-,6.8 ~ 16.8 ~ 18.7,ZBNW60GM3A0,43.5,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,2.5,66,42 / 40 / 38,-,Duct Mid Static

