,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"ZUUW24GA0","UU24WR U40",U4,"1,500 x 1",Twin Rotary,-,2.84 ~ 6.80 ~ 7.80,-,950 x 834 x 330,Electronic Expansion Valve,-,58 x 1,124 x 1,BLDC,Axial,-,3.20 ~ 8.00 ~ 8.80,ZUUW24GA0,56.1,-,5/8,15.88 ,3/8,9.52,0.32 ~ 1.94 ~ 2.73,0.32 ~ 2.00 ~ 3.20,"1 , 220-240 , 50",3C x 2.5,1600,15.88 ,9.52,R32,8.6,8.8,67,-,48,52,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC Standard Inverter
"ZUUW30GA0","UU30WR U40",U4,"2,020 x 1",Twin Rotary,-,3.2 ~ 8.0 ~ 9.5,-,950 x 834 x 330,Electronic Expansion Valve,-,58 × 1,124 × 1,BLDC,Axial,-,3.6 ~ 9.0 ~ 9.9,ZUUW30GA0 ,57.3,-,5/8,15.88 ,3/8,9.52,0.25 ~ 2.39 ~ 3.05,0.28 ~ 2.40 ~ 3.20,"1 , 220-240 , 50",3C × 2.5,1900,15.88 ,9.52,R32,10.6,10.6,68,68,50,52,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC Standard Inverter
"ZUUW36GC0","UU36WCR U40",U4,"2,020 x 1",Twin Rotary,-,3.8 ~ 9.5 ~ 10.6,-,950 x 834 x 330,Electronic Expansion Valve,-,70 x 1,124 x 1,BLDC,Axial,-,4.0 ~ 10.8 ~ 11.4,ZUUW36GC0 ,57.3,-,5/8,15.88 ,3/8,9.52,0.28 ~ 3.16 ~ 3.26,0.39 ~ 3.09 ~ 3.37,"1 , 220-240 , 50",3C × 2.5,1900,15.88 ,9.52,R32,14,13.7,70,70,54,56,-10~48,14 ~ 118.4,-10~25,14 ~77,SingleCAC Compact Inverter

