,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ZBNW36GM2A0","UM36R N20",-,32 / 28 / 24,M2,32,-,4.5 ~ 9.5 ~ 13.0,-,"1,250 x 270 x 700",295 x 1,BLDC,Sirocco Fan,-,5.0 ~ 10.8 ~ 13.7,ZBNW36GM2A0,38.5,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,2.5,60,36 / 34 / 33,-,Duct Mid Static
"ZBNW42GM2A0","UM42R N20",-,38 / 33 / 28,M2,32,-,5.0 ~ 12.0 ~ 14.5,-,"1,250 x 270 x 700",295 x 1,BLDC,Sirocco Fan,-,5.5 ~ 13.5 ~ 16.5,ZBNW42GM2A0,38.5,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,2.5,62,38 / 36 / 34,-,Duct Mid Static

