,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"S3NM18KL1ZA",DC18RQ NSK,501 / 399 / 350,14.2 / 11.3 /9.9,SK,21.5,-,5,39-9/32 x 13-19/32 x 8-9/32,998 x 345 x 210,60 x 1,BLDC,Cross Flow Fan,-,5.8,S3NM18KL1ZA,12,26.5,-,21.5,1/2,12.7 ,1/4,6.35 ,4C x 1.0 (18),26 / 39 / 60,-,"1,220-240, 50 / 1, 220, 60",12.7 ,6.35 ,R32,0.22 / 0.28 / 0.40,60,44 / 38 / 35,44 / 38 / 35,Wall Mounted(2)
"S3NM18KL2FA",PC18SQ NSK,501 / 399 / 350 ,14.2 / 11.3 / 9.9,SK,21.5,-,5,39-9/32 x 13-19/32 x 8-9/32,998 x 345 x 210,60 x 1,BLDC,Cross Flow Fan,-,5.8,S3NM18KL2FA,12,26.5,-,21.5,1/2,12.7 ,1/4,6.35 ,4C x 0.75 (18),26 / 39 / 60,-,"1,220-240, 50 / 1, 220, 60",12.7 ,6.35 ,R32,0.22 / 0.28 / 0.40,59,44 / 38 / 35,44 / 38 / 35,Wall Mounted(2)
"S3NM18KL3BA",SC18EQ NSK,501 / 399 / 350 ,14.2 / 11.3 / 9.9,SK,21.5,-,5,39-9/32 x 13-19/32 x 8-9/32,998 x 345 x 210,60 x 1,BLDC,Cross Flow Fan,-,5.8,S3NM18KL3BA,12,26.5,-,21.5,1/2,12.7 ,1/4,6.35 ,4C x 0.75 (18),26 / 39 / 60,-,"1,220-240, 50 / 1, 220, 60",12.7 ,6.35 ,R32,0.22 / 0.28 / 0.40,59,44 / 38 / 35,44 / 38 / 35,Wall Mounted(2)

