,Model name (Buyer)##other##,URL##OTHER##,Type##OTHER##,Sound Pressure Level Heating(dB)##OTHER##,Sound Pressure Level Cooling(dB)##OTHER##,Sound Power Level (dB(A))##OTHER##,Running Current (A)##OTHER##,Refrigerant Type##OTHER##,Refrigerant Gas Connection Radius##LENGTH##MILLIMETERS,Refrigerant Liquid Connection Radius##LENGTH##MILLIMETERS,Refrigerant Liquid Connection Diameter##PIPE_SIZE##MILLIMETERS,Refrigerant Gas Connection Diameter##PIPE_SIZE##MILLIMETERS,Power and Communication Cable##OTHER##,Power Supply (Ph_V_Hz)##OTHER##,Power Input (Heating)(W)##OTHER##,Power Input (Cooling)(W)##OTHER##,Pipe Connection_Liquid Side (mm)##OTHER##,Pipe Connection_Liquid Side (inch)##OTHER##,Pipe Connection_Gas Side (mm)##OTHER##,Pipe Connection_Gas Side (inch)##OTHER##,Pipe Connection_Drain Side (mm)##OTHER##,Pipe Connection_Drain Side (inch)##OTHER##,Net Weight (lbs)##OTHER##,Net Weight (kg)##OTHER##,Model name (Factory)##OTHER##,Heating Capacity (kW)##OTHER##,Heating Capacity (Btu/h)##OTHER##,Fan Type##OTHER##,Fan Motor Type##OTHER##,Fan Motor Output (W)##OTHER##,Dimensions (WxHxD)(mm)##OTHER##,Dimensions (WxHxD)(inch)##OTHER##,Cooling Capacity (kW)##OTHER##,Cooling Capacity (Btu/h)##OTHER##,Condensate Drain Connection Radius##LENGTH##MILLIMETERS,Condensate Drain Connection Diameter##PIPE_SIZE##MILLIMETERS,Chassis name##OTHER##,Air Flow Rate (H/M/L)(CMM)##OTHER##,Air Flow Rate (H/M/L)(CFM)##OTHER##
"ZVNW18GM1A0","UV18R N10",http://partner.lge.com/global,Ceiling Suspended,-,42 / 40 / 39,55,1,R32,6.35,3.175000000000,6.35,12.70,4C x 0.75,"1, 220-240, 50 / 1, 220, 60",-,23,6.35,1/4,12.7,1/2,21.5,-,-,27.3,ZVNW18GM1A0,5.20,"17.743",Cross flow Fan,BLDC,105.4 x 1,"1,200 x 235 x 690",-,5.00,"17,060",10.750000000000,21.500000000000,VM1,13.0 / 12.0 / 11.0,-
"ZVNW24GM1A0","UV24R N10",http://partner.lge.com/global,Ceiling Suspended,-,46 / 45 / 43,61,1,R32,7.94,4.760000000000,9.52,15.88,4C x 0.75,"1, 220-240, 50 / 1, 220, 60",-,26,9.52,3/8,15.88,5/8,21.5,-,-,28,ZVNW24GM1A0,7.50,"25,591",Cross flow Fan,BLDC,105.4 x 1,"1,200 x 235 x 690",-,6.80,"23,202",10.750000000000,21.500000000000,VM1,16.0 / 15.0 / 14.0,-
"ZVNW30GM1A0","UV30R N10",http://partner.lge.com/global,Ceiling Suspended,-,46 / 44 / 43,62,1,R32,7.94,4.760000000000,9.52,15.88,4C x 0.75,"1, 220-240, 50 / 1, 220, 60",-,40,9.52,3/8,15.88,5/8,21.5,-,-,28,ZVNW30GM1A0,8.00,"27,297",Cross flow Fan,BLDC,85.9 x 1,"1,200 x 235 x 690",-,7.50,"25,591",10.750000000000,21.500000000000,VM1,19.0 / 17.5 / 16.0,-