,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ZBNW09GL2A0","CL09R N20",-,10.0 / 8.5 / 7.0,L2,32,-,1.10 ~ 2.50 ~ 3.20,-,900 × 190 × 700,19 × 1 + 5 × 1,BLDC,Sirocco,-,1.20 ~ 3.20 ~ 3.60,ZBNW09GL2A0,24,-,-,32,3/8,9.52 ,1/4,6.35 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",9.52 ,6.35 ,R32,0.8,55,31 / 28 / 27,-,Duct Low Static
"ZBNW12GL2A0","CL12R N20",-,10.0 / 8.5 / 7.0,L2,32,-,1.40 ~ 3.40 ~ 3.90,-,900 × 190 × 700,19 × 1 + 5 × 1,BLDC,Sirocco,-,1.60 ~ 4.00 ~ 4.70,ZBNW12GL2A0,24,-,-,32,3/8,9.52 ,1/4,6.35 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",9.52 ,6.35 ,R32,0.8,55,31 / 28 / 27,-,Duct Low Static
"ZBNW18GL2A0","CL18R N20",-,15.0 / 12.5 / 10.0,L2,32,-,2.00 ~ 5.00 ~ 6.00,-,900 × 190 × 700,19 x 1 + 5 x 1,BLDC,Sirocco,-,2.20 ~ 6.00 ~ 7.20,ZBNW18GL2A0,24,-,-,32,1/2,12.7 ,1/4,6.35 ,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",12.7 ,6.35 ,R32,0.8,54,36 / 34 / 31,-,Duct Low Static

