,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AUUW18GC0","UU18WC UL0",UL2,"1,500 x 1",Twin Rotary,"6,140 ~ 16,040 ~ 17,410",1.80 ~ 4.70 ~ 5.10,30-5/16 x 21-15/32 x 11-11/32,770 x 545 x 288,Electronic Expansion Valve,988.85 x 1,28 x 1,43.0 x 1,BLDC,Axial,"5,800 ~ 17,750 ~ 19,460",1.70 ~ 5.20 ~ 5.70,AUUW18GC0,37.5 ,82.6,1/2,12.7,1/4,6.35,1.63,1.67,"1, 220-240, 50",5C x 2.5 (12),"1,300 ",12.7,6.35,R410A,7.3,7.4,65,-,47,49,-10 ~ 48,14 ~ 118.4,-10 ~ 18,14 ~ 64.4,SingleCAC_CompactInverter
"AUUW24GC0","UU24WC UE0",UL2,"1,500 x 1",Twin Rotary,"9,210 ~ 23,210 ~ 25,260",2.70 ~ 6.80 ~ 7.40,34-1/4 x 25-25/32 x 12-19/32,870 x 655 x 320,Electronic Expansion Valve,1765.8 x 1,50 x 1,85.4 x 1,BLDC,Axial,"6,480 ~ 25,600 ~ 28,000",1.90 ~ 7.50 ~ 8.20,AUUW24GC0,44.5 ,98.1,5/8,15.88,3/8,9.52,2.33,2.4,"1, 220-240, 50",5C x 2.5 (12),"1,400 ",15.88,9.52,R410A,9.4,9.6,68,-,48,50,-10 ~ 48,14 ~ 118.4,-15 ~ 18,5 ~ 64.4,SingleCAC_CompactInverter

