,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AUUW30GC0","UU30WC UE0",UE,"1,500 x 1",Twin Rotary,"10,900 ~ 25,600 ~ 26,600",3.20~ 7.50 ~ 7.80,34-1/4 x 25-25/32 x 12-19/32,870 x 655 x 320,Electronic Expansion Valve,1765.8 x 1,50 x 1,85.4 x 1,BLDC,Axial,"12,300 ~ 27,300 ~ 30,000",3.60 ~ 8.00 ~ 8.80,AUUW30GC0,45.4 ,100,5/8,15.88,3/8,9.52,2.68,2.25,"1, 220-240, 50",3C x 2.5 (14),"1,600 ",15.88,9.52,R410A,12,10,70,-,51,52,-10 ~ 48,14 ~ 118.4,-10 ~ 18,14 ~ 64.4,SingleCAC_CompactInverter
"AUUW36GC0","UU36WC U40",UE,"2,137 x 1",Twin Rotary,"13,000 ~ 32,400 ~ 34,100",3.80 ~ 9.50 ~ 10.0,37-13/32 x 32-27/32 x 13,950 x 834 x 330,Electronic Expansion Valve,2048.33 x 1,58 x 1,124.0 x 1,BLDC,Axial,"13,600 ~ 34,100 ~ 35,800",4.00 ~ 10.0 ~ 10.50,AUUW36GC0,58.2 ,128.3,5/8,15.88,3/8,9.52,3.35,2.93,"1, 220-240, 50",3C x 2.5 (14),"2,200 ",15.88,9.52,R410A,14.9,13,70,-,54,56,-10 ~ 48,14 ~ 118.4,-10 ~ 18,14 ~ 64.4,SingleCAC_CompactInverter

