,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
UUB1 U20,UUB1 U20,U24A,"1,500 x 1",Twin Rotary,-,2.0 ~ 5.0 ~ 5.8 (IDU :  MJ18PC),34-1/4 x 25-19/32 x 12-63/64,870 x 650 x 330,Electronic Expansion Valve,1765 x 1,50 x 1,85.4 x 1,BLDC,Propeller,-,2.30 ~ 5.80 ~ 6.10 (IDU : MJ18PC),ZUUW24GA1,44.5,98.1,1/2,12.7 ,1/4,6.35 ,0.30 ~ 1.33 ~ 1.86,0.40 ~ 1.76 ~ 2.46,"1 , 220-240 , 50",3C x 2.5,1200,12.7 ,6.35 ,R32,7.4,8.3,63,-,47,52,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC_Free_Combi
