,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AUUW09GA0","UU09W UL0",UL2,"1,500 x 1",Twin Rotary,"3,400 ~ 8,500 ~ 9,400",1.00 ~ 2.50 ~ 2.75,-,870 x 655 x 320,Electronic Expansion Valve,988.8 x 1,28 x 1,43.0 x 1,BLDC,Axial,"4,100 ~ 10,200 ~ 11,300",1.20 ~ 3.00 ~ 3.30,AUUW09GA0,46,98.3,3/8,9.52,1/4,6.35,0.625,0.8,"1, 220-240, 50",3C x 2.5 (12),1300,9.52,6.35,R410A,2.7,3.5,65,-,47,50,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 18,SingleCAC_StandardInverter
"AUUW12GA0","UU12W UL0",UL2,"1,500 x 1",Twin Rotary,"4,600 ~ 11,600 ~ 12,800",1.36 ~ 3.40 ~ 3.74,-,770 x 545 x 288,Electronic Expansion Valve,988.8 x 1,28 x 1,43.0 x 1,BLDC,Axial,"5,500 ~ 13,600 ~ 15,000",1.60 ~ 4.00 ~ 4.40,AUUW12GA0,33.8,74.5,3/8,9.52,1/4,6.35,0.97,1.15,"1, 220-240, 50",3C x 2.5 (12),1100,9.52,6.35,R410A,4.3,5,65,-,49,52,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 18,SingleCAC_StandardInverter

