,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
S3NM09JASZA,AC09SQ NSJ,441 / 353 / 265 / 148,12.5 / 10.0 / 7.5 / 4.2,SJ,21.5,-,2.5,32-15/16 x 12-1/8 x 7-9/16,837 x 308 x 192,30 x 1,BLDC,Cross Flow Fan,-,3.3,S3NM09JASZA,9.9,21.8,-,21.5,3/8,9.52 ,1/4,6.35 ,4C x 1.0,11 / 18 / 30,-,"1,220-240, 50",9.52 ,6.35 ,R32,0.10 / 0.16 / 0.20,59,41 / 35 / 27,41 / 35 / 27,Artcool Silver
S3NM12JASZA,AC12SQ NSJ,441 / 353 / 265 / 148,12.5 / 10.0 / 7.5 / 4.2,SJ,21.5,-,3.5,32-15/16 x 12-1/8 x 7-9/16,837 x 308 x 192,30 x 1,BLDC,Cross Flow Fan,-,4,S3NM12JASZA,9.9,21.8,-,21.5,3/8,9.52 ,1/4,6.35 ,4C x 1.0,11 / 19 / 30,-,"1,220-240, 50",9.52 ,6.35 ,R32,0.10 / 0.17 / 0.20,59,41 / 35 / 27,41 / 35 / 27,Artcool Silver