,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ZVNW36GM2A0","UV36R N20",-,28 / 24 / 20,VM2,32,-,4.5 ~ 9.5 ~ 13.0,-,"1,600 x 235 x 690",124 x 1,BLDC,Cross Flow Fan,-,5.0 ~ 10.8 ~ 13.7,ZVNW36GM2A0,36.5,-,-,32,5/8,15.88,3/8,9.52,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.47,63,46 / 43 / 40,-,Ceiling Suspended
"ZVNW42GM2A0","UV42R N20",-,28 / 24 / 20,VM2,32,-,5.0 ~ 12.0 ~ 14.5,-,"1,600 x 235 x 690",124 x 1,BLDC,Cross Flow Fan,-,5.5 ~ 13.5 ~ 16.5,ZVNW42GM2A0,36.5,-,-,32,5/8,15.88,3/8,9.52,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.47,63,46 / 43 / 40,-,Ceiling Suspended
"ZVNW48GM2A0","UV48R N20",-,30 / 25 / 20,VM2,32,-,5.5 ~ 13.4 ~ 16.0,-,"1,600 x 235 x 690",124 x 1,BLDC,Cross Flow Fan,-,6.1 ~ 15.5 ~ 18.0,ZVNW48GM2A0,36.5,-,-,32,5/8,15.88,3/8,9.52,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.47,63,48 / 44 / 40,-,Ceiling Suspended
"ZVNW60GM2A0","UV60R N20",-,30 / 25 / 20,VM2,32,-,5.7 ~ 14.4 ~ 15.7,-,"1,600 x 235 x 690",124 x 1,BLDC,Cross Flow Fan,-,6.8 ~ 16.8 ~ 18.7,ZVNW60GM2A0,36.5,-,-,32,5/8,15.88,3/8,9.52,4C x 0.75,-,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.47,63,48 / 44 / 40,-,Ceiling Suspended

