,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ZMNW18GSKC0",MJ18PC NSK,558 / 438 / 353,15.8 / 12.4 / 10.0,SK,21.5,-,5.3,38-3/8 x 13-15/16 x 8-7/32,975 x 354 x 209,30 x 1,BLDC,Cross Flow Fan,-,6.3,ZMNW18GSKC0,10.9,24,-,21.5,1/2,12.7 ,1/4,6.35 ,4C x 0.75 (18),26 / 39 / 60,-,"1,220-240, 50 / 1, 220, 60",12.7 ,6.35 ,R32,0.22 / 0.28 / 0.40,59,44 / 38 / 34,44 / 38 / 34,Wall Mounted(3)
"ZMNW24GSKC0",MJ24PC NSK,597 / 452 / 367,16.9 / 12.8 / 10.4,SK,21.5,-,7,38-3/8 x 13-15/16 x 8-7/32,975 x 354 x 209,60 x 1,BLDC,Cross Flow Fan,-,7.5,ZMNW24GSKC0,11.5,25.4,-,21.5,1/2,12.7 ,1/4,6.35 ,4C x 0.75 (18),27 / 45 / 60,-,"1,220-240, 50 / 1, 220, 60",12.7 ,6.35 ,R32,0.24 / 0.33 / 0.40,65,46 / 41 / 36,46 / 41 / 36,Wall Mounted(3)

