,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"ZUUW18GA0","UU18WR U20",U24A,"1,500 x 1",Twin Rotary,-,2.00 ~ 5.00 ~ 5.75,-,870 x 650 x 330,Electronic Expansion Valve,-,50 x 1,85.4 x 1,BLDC,Axial,-,2.20 ~ 5.80 ~ 6.80,ZUUW18GA0,44.8,-,1/2,12.7 ,1/4,6.35 ,0.30 ~ 1.56 ~ 2.50,0.28 ~ 1.66 ~ 2.66,"1 , 220-240 , 50",3C x 2.5,1100,12.7 ,6.35 ,R32,7.1,7.5,63,-,47,52,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC Standard Inverter
"ZUUW24GC0","UU24WCR U20",U24A,"1,500 x 1",Twin Rotary,-,2.7 / 6.8 / 7.4,-,870 x 650 x 330,Electronic Expansion Valve,-,50 x 1,85.4 x 1,BLDC,Axial,-,1.9 / 7.5 / 8.2,ZUUW24GC0,45,-,5/8,15.88 ,3/8,9.52,0.16 ~ 2.27 ~ 2.80,0.40 ~ 2.40 ~ 2.76,"1 , 220-240 , 50",3C x 2.5,1300,15.88 ,9.52,R32,10.2,10.6,65,-,48,53,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC Compact Inverter
"ZUUW30GC0","UU30WCR U20",U24A,"1,500 x 1",Twin Rotary,-,3.0 / 7.5 / 8.2,-,870 x 650 x 330,Electronic Expansion Valve,-,50 x 1,85.4 x 1,BLDC,Axial,-,2.0 / 8.0 / 8.4,ZUUW30GC0,45,-,5/8,15.88 ,3/8,9.52,  0.20 ~ 2.34 ~2.90,0.50 ~2.28 ~ 2.40,"1 , 220-240 , 50",3C x 2.5,1300,15.88 ,9.52,R32,10.6,10,67,-,50,54,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC Compact Inverter

