,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
S3NM24K22FA,PC24SQ NSK, 569 / 463 / 371,16.1 / 13.1 / 10.5,SK,21.5,-,6.6,39-9/32 x 13-19/32 x 8-9/32,998 x 345 x 210,58 x 1,BLDC,Cross Flow Fan,-,7.5,S3NM24K22FA,12.7,28,-,21.5,5/8,15.88,1/4,6.35 ,4C x 1.0 (18),27 / 45 / 60,-,"1, 220-240, 50",15.88,6.35 ,R32,0.24 / 0.33 / 0.40,65,47/ 42 / 34,47 / 42 / 34,Wall Mounted
S3NM24K21ZA,DC24RQ NSK,569 / 463 / 371,16.1 / 13.1 / 10.5,SK,21.5,-,6.6,39-9/32 x 13-19/32 x 8-9/32,998 x 345 x 210,58 x 1,BLDC,Cross Flow Fan,-,7.5,S3NM24K21ZA,12.7,28,-,21.5,5/8,15.88,1/4,6.35 ,4C x 1.0 (18),27 / 45 / 60,-,"1, 220-240, 50",15.88,6.35 ,R32,0.24 / 0.33 / 0.40,65,47/ 42 / 34,47 / 42 / 34,Wall Mounted
