,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"ZUUW09GA0","UU09WR UL0",UL2,"1,500 x 1",Twin Rotary,-,1.00 ~ 2.50 ~ 2.87,-,770 x 545 x 288,Electronic Expansion Valve,-,28 x 1,43.0 x 1,BLDC,Axial,-,1.20 ~ 3.20 ~ 3.45,ZUUW09GA0,33.8,-,3/8,9.52 ,1/4,6.35 ,0.11 ~ 0.63 ~ 0.99,0.18 ~ 0.75 ~ 1.20,"1 , 220-240 , 50",3C x 2.5,900,9.52 ,6.35 ,R32,2.7,3.5,65,-,47,50,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC Standard Inverter
"ZUUW12GA0","UU12WR UL0",UL2,"1,500 x 1",Twin Rotary,-,1.36 ~ 3.40 ~ 3.90,-,770 x 545 x 288,Electronic Expansion Valve,-,28 x 1,43.0 x 1,BLDC,Axial,-,1.60 ~ 4.00 ~ 4.6,ZUUW12GA0,33.8,-,3/8,9.52 ,1/4,6.35 ,0.11 ~ 0.97 ~ 1.55,0.18 ~ 1.12 ~ 1.79,"1 , 220-240 , 50",3C x 2.5,900,9.52 ,6.35 ,R32,4.3,5,65,-,49,52,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC Standard Inverter
"ZUUW18GC0","UU18WCR UL0",UL2,"1,500 x 1",Twin Rotary,-,1.80 ~ 5.00 ~ 5.30,-,770 x 545 x 288,Electronic Expansion Valve,-,28 x 1,43.0 x 1,BLDC,Axial,-,1.70 ~ 5.20 ~ 6.00,ZUUW18GC0,34.5,-,1/2,12.7 ,1/4,6.35 ,0.14~ 1.67 ~ 1.80,0.23 ~ 1.58 ~2.08,"1 , 220-240 , 50",3C x 2.5,1000,12.7 ,6.35 ,R32,7.4,7,65,-,49,52,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC Compact Inverter

