,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"UVNH36GKLA2","UV36 NK2",756 / 699 / 643,21.4 / 19.8 / 18.2,VK,21.5,"13,000 ~ 32,400 ~ 35,800",3.80 ~ 9.50 ~ 10.5,53-5/32 x 25-19/32 x 8-21/32,"1,350 x 650 x 220",43.1 x 2,BLDC,Cross flow Fan,"14,300 ~ 35,800 ~ 39,600",4.20 ~ 10.5 ~ 11.6,UVNH36GKLA2,34.1,75.2,27/32,21.5,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),40 / 90,-,"1, 220-240, 50 / 1, 230, 60",15.88,9.52,R410A,0.7,63,45 / 44 / 41,-,Convertible

